**Control Switch Assembly**

Single pole/single throw, single pole/double throw and double pole/double throw toggle switches with stainless steel switch plate and indicator lights. Available in single and multiple gang configurations.

**Technical Specifications**

|  |  |
| --- | --- |
| **Construction** | Switch: toggle switch with pre-wired pigtails  Switch Plate: Stamped stainless-steel switch plate pre-punched for switch(es) Indicator light(s): Available in red, green or amber |
| **Finish** | Switch plate brushed stainless steel |
| **Electrical** | 120VAC, 277VAC, 12VDC, 24VDC |
| **Dimensions** | 4.5”H x varied width x 1”D X length varies on gang configuration |
| **Compatible** | All sign series |

**Control Switch Customization Choices**

|  |  |
| --- | --- |
| **Switch Assembly Configurations** | Any combination of single pole single throw, single pole double throw and double pole double throw switches up to an 8-gang configuration. |
| **Custom Switch Plate** | Switch plate pre-punched to fit gang configuration |
| **Indicator Lights** | Any combination of light colors available |

|  |
| --- |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |
|  |